\hypertarget{class_nex_radio}{\section{Nex\+Radio Class Reference}
\label{class_nex_radio}\index{Nex\+Radio@{Nex\+Radio}}
}


{\ttfamily \#include $<$Nex\+Radio.\+h$>$}

Inheritance diagram for Nex\+Radio\+:\begin{figure}[H]
\begin{center}
\leavevmode
\includegraphics[height=3.000000cm]{class_nex_radio}
\end{center}
\end{figure}
\subsection*{Public Member Functions}
\begin{DoxyCompactItemize}
\item 
\hyperlink{class_nex_radio_a52264cd95aaa3ba7b4b07bdf64bb7a65}{Nex\+Radio} (uint8\+\_\+t pid, uint8\+\_\+t cid, const char $\ast$name)
\item 
uint32\+\_\+t \hyperlink{class_nex_radio_adb3672f10ce98ec7ad22f7b29a9ec0e6}{get\+Value} (uint32\+\_\+t $\ast$number)
\item 
bool \hyperlink{class_nex_radio_aa92d6f41ff30467a965e8a802e7d8b83}{set\+Value} (uint32\+\_\+t number)
\item 
uint32\+\_\+t \hyperlink{class_nex_radio_abdc8f654237d900eb3ddc955bc9e0038}{Get\+\_\+background\+\_\+color\+\_\+bco} (uint32\+\_\+t $\ast$number)
\item 
bool \hyperlink{class_nex_radio_a7bbd252dc78876d0831badbe791dbbc8}{Set\+\_\+background\+\_\+color\+\_\+bco} (uint32\+\_\+t number)
\item 
uint32\+\_\+t \hyperlink{class_nex_radio_a7a052fb745dfea5fe6f341692eb0ca1a}{Get\+\_\+font\+\_\+color\+\_\+pco} (uint32\+\_\+t $\ast$number)
\item 
bool \hyperlink{class_nex_radio_afd379837becbcf4a8f126820658a7f78}{Set\+\_\+font\+\_\+color\+\_\+pco} (uint32\+\_\+t number)
\end{DoxyCompactItemize}
\subsection*{Additional Inherited Members}


\subsection{Detailed Description}
\hyperlink{class_nex_radio}{Nex\+Radio} component.

Commonly, you want to do something after push and pop it. It is recommanded that only call \hyperlink{class_nex_touch_a4da1c4fcdfadb7eabfb9ccaba9ecad11}{Nex\+Touch\+::attach\+Pop} to satisfy your purpose.

\begin{DoxyWarning}{Warning}
Please do not call \hyperlink{class_nex_touch_a685a753aae5eb9fb9866a7807a310132}{Nex\+Touch\+::attach\+Push} on this component, even though you can. 
\end{DoxyWarning}


\subsection{Constructor \& Destructor Documentation}
\hypertarget{class_nex_radio_a52264cd95aaa3ba7b4b07bdf64bb7a65}{\index{Nex\+Radio@{Nex\+Radio}!Nex\+Radio@{Nex\+Radio}}
\index{Nex\+Radio@{Nex\+Radio}!Nex\+Radio@{Nex\+Radio}}
\subsubsection[{Nex\+Radio}]{\setlength{\rightskip}{0pt plus 5cm}Nex\+Radio\+::\+Nex\+Radio (
\begin{DoxyParamCaption}
\item[{uint8\+\_\+t}]{pid, }
\item[{uint8\+\_\+t}]{cid, }
\item[{const char $\ast$}]{name}
\end{DoxyParamCaption}
)}}\label{class_nex_radio_a52264cd95aaa3ba7b4b07bdf64bb7a65}




Constructor.


\begin{DoxyParams}{Parameters}
{\em pid} & -\/ page id. \\
\hline
{\em cid} & -\/ component id. \\
\hline
{\em name} & -\/ pointer to an unique name in range of all components. \\
\hline
\end{DoxyParams}


\subsection{Member Function Documentation}
\hypertarget{class_nex_radio_abdc8f654237d900eb3ddc955bc9e0038}{\index{Nex\+Radio@{Nex\+Radio}!Get\+\_\+background\+\_\+color\+\_\+bco@{Get\+\_\+background\+\_\+color\+\_\+bco}}
\index{Get\+\_\+background\+\_\+color\+\_\+bco@{Get\+\_\+background\+\_\+color\+\_\+bco}!Nex\+Radio@{Nex\+Radio}}
\subsubsection[{Get\+\_\+background\+\_\+color\+\_\+bco}]{\setlength{\rightskip}{0pt plus 5cm}uint32\+\_\+t Nex\+Radio\+::\+Get\+\_\+background\+\_\+color\+\_\+bco (
\begin{DoxyParamCaption}
\item[{uint32\+\_\+t $\ast$}]{number}
\end{DoxyParamCaption}
)}}\label{class_nex_radio_abdc8f654237d900eb3ddc955bc9e0038}
Get bco attribute of component


\begin{DoxyParams}{Parameters}
{\em number} & -\/ buffer storing data retur \\
\hline
\end{DoxyParams}
\begin{DoxyReturn}{Returns}
the length of the data 
\end{DoxyReturn}
\hypertarget{class_nex_radio_a7a052fb745dfea5fe6f341692eb0ca1a}{\index{Nex\+Radio@{Nex\+Radio}!Get\+\_\+font\+\_\+color\+\_\+pco@{Get\+\_\+font\+\_\+color\+\_\+pco}}
\index{Get\+\_\+font\+\_\+color\+\_\+pco@{Get\+\_\+font\+\_\+color\+\_\+pco}!Nex\+Radio@{Nex\+Radio}}
\subsubsection[{Get\+\_\+font\+\_\+color\+\_\+pco}]{\setlength{\rightskip}{0pt plus 5cm}uint32\+\_\+t Nex\+Radio\+::\+Get\+\_\+font\+\_\+color\+\_\+pco (
\begin{DoxyParamCaption}
\item[{uint32\+\_\+t $\ast$}]{number}
\end{DoxyParamCaption}
)}}\label{class_nex_radio_a7a052fb745dfea5fe6f341692eb0ca1a}
Get pco attribute of component


\begin{DoxyParams}{Parameters}
{\em number} & -\/ buffer storing data retur \\
\hline
\end{DoxyParams}
\begin{DoxyReturn}{Returns}
the length of the data 
\end{DoxyReturn}
\hypertarget{class_nex_radio_adb3672f10ce98ec7ad22f7b29a9ec0e6}{\index{Nex\+Radio@{Nex\+Radio}!get\+Value@{get\+Value}}
\index{get\+Value@{get\+Value}!Nex\+Radio@{Nex\+Radio}}
\subsubsection[{get\+Value}]{\setlength{\rightskip}{0pt plus 5cm}uint32\+\_\+t Nex\+Radio\+::get\+Value (
\begin{DoxyParamCaption}
\item[{uint32\+\_\+t $\ast$}]{number}
\end{DoxyParamCaption}
)}}\label{class_nex_radio_adb3672f10ce98ec7ad22f7b29a9ec0e6}
Get val attribute of component


\begin{DoxyParams}{Parameters}
{\em number} & -\/ buffer storing data retur \\
\hline
\end{DoxyParams}
\begin{DoxyReturn}{Returns}
the length of the data 
\end{DoxyReturn}
\hypertarget{class_nex_radio_a7bbd252dc78876d0831badbe791dbbc8}{\index{Nex\+Radio@{Nex\+Radio}!Set\+\_\+background\+\_\+color\+\_\+bco@{Set\+\_\+background\+\_\+color\+\_\+bco}}
\index{Set\+\_\+background\+\_\+color\+\_\+bco@{Set\+\_\+background\+\_\+color\+\_\+bco}!Nex\+Radio@{Nex\+Radio}}
\subsubsection[{Set\+\_\+background\+\_\+color\+\_\+bco}]{\setlength{\rightskip}{0pt plus 5cm}bool Nex\+Radio\+::\+Set\+\_\+background\+\_\+color\+\_\+bco (
\begin{DoxyParamCaption}
\item[{uint32\+\_\+t}]{number}
\end{DoxyParamCaption}
)}}\label{class_nex_radio_a7bbd252dc78876d0831badbe791dbbc8}
Set bco attribute of component


\begin{DoxyParams}{Parameters}
{\em number} & -\/ To set up the data \\
\hline
\end{DoxyParams}
\begin{DoxyReturn}{Returns}
true if success, false for failure 
\end{DoxyReturn}
\hypertarget{class_nex_radio_afd379837becbcf4a8f126820658a7f78}{\index{Nex\+Radio@{Nex\+Radio}!Set\+\_\+font\+\_\+color\+\_\+pco@{Set\+\_\+font\+\_\+color\+\_\+pco}}
\index{Set\+\_\+font\+\_\+color\+\_\+pco@{Set\+\_\+font\+\_\+color\+\_\+pco}!Nex\+Radio@{Nex\+Radio}}
\subsubsection[{Set\+\_\+font\+\_\+color\+\_\+pco}]{\setlength{\rightskip}{0pt plus 5cm}bool Nex\+Radio\+::\+Set\+\_\+font\+\_\+color\+\_\+pco (
\begin{DoxyParamCaption}
\item[{uint32\+\_\+t}]{number}
\end{DoxyParamCaption}
)}}\label{class_nex_radio_afd379837becbcf4a8f126820658a7f78}
Set pco attribute of component


\begin{DoxyParams}{Parameters}
{\em number} & -\/ To set up the data \\
\hline
\end{DoxyParams}
\begin{DoxyReturn}{Returns}
true if success, false for failure 
\end{DoxyReturn}
\hypertarget{class_nex_radio_aa92d6f41ff30467a965e8a802e7d8b83}{\index{Nex\+Radio@{Nex\+Radio}!set\+Value@{set\+Value}}
\index{set\+Value@{set\+Value}!Nex\+Radio@{Nex\+Radio}}
\subsubsection[{set\+Value}]{\setlength{\rightskip}{0pt plus 5cm}bool Nex\+Radio\+::set\+Value (
\begin{DoxyParamCaption}
\item[{uint32\+\_\+t}]{number}
\end{DoxyParamCaption}
)}}\label{class_nex_radio_aa92d6f41ff30467a965e8a802e7d8b83}
Set val attribute of component


\begin{DoxyParams}{Parameters}
{\em number} & -\/ To set up the data \\
\hline
\end{DoxyParams}
\begin{DoxyReturn}{Returns}
true if success, false for failure 
\end{DoxyReturn}


The documentation for this class was generated from the following files\+:\begin{DoxyCompactItemize}
\item 
\hyperlink{_nex_radio_8h}{Nex\+Radio.\+h}\item 
\hyperlink{_nex_radio_8cpp}{Nex\+Radio.\+cpp}\end{DoxyCompactItemize}
