<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<settings>
<setting alwaysvectorfont="no"/>
<setting verticaltext="up"/>
</settings>
<grid distance="0.1" unitdist="inch" unit="inch" style="lines" multiple="1" display="no" altdistance="0.01" altunitdist="inch" altunit="inch"/>
<layers>
<layer number="1" name="Top" color="4" fill="1" visible="yes" active="yes"/>
<layer number="16" name="Bottom" color="1" fill="1" visible="yes" active="yes"/>
<layer number="17" name="Pads" color="2" fill="1" visible="yes" active="yes"/>
<layer number="18" name="Vias" color="2" fill="1" visible="yes" active="yes"/>
<layer number="19" name="Unrouted" color="6" fill="1" visible="yes" active="yes"/>
<layer number="20" name="Dimension" color="15" fill="1" visible="yes" active="yes"/>
<layer number="21" name="tPlace" color="7" fill="1" visible="yes" active="yes"/>
<layer number="22" name="bPlace" color="7" fill="1" visible="yes" active="yes"/>
<layer number="23" name="tOrigins" color="15" fill="1" visible="yes" active="yes"/>
<layer number="24" name="bOrigins" color="15" fill="1" visible="yes" active="yes"/>
<layer number="25" name="tNames" color="7" fill="1" visible="yes" active="yes"/>
<layer number="26" name="bNames" color="7" fill="1" visible="yes" active="yes"/>
<layer number="27" name="tValues" color="7" fill="1" visible="yes" active="yes"/>
<layer number="28" name="bValues" color="7" fill="1" visible="yes" active="yes"/>
<layer number="29" name="tStop" color="7" fill="3" visible="no" active="yes"/>
<layer number="30" name="bStop" color="7" fill="6" visible="no" active="yes"/>
<layer number="31" name="tCream" color="7" fill="4" visible="no" active="yes"/>
<layer number="32" name="bCream" color="7" fill="5" visible="no" active="yes"/>
<layer number="33" name="tFinish" color="6" fill="3" visible="no" active="yes"/>
<layer number="34" name="bFinish" color="6" fill="6" visible="no" active="yes"/>
<layer number="35" name="tGlue" color="7" fill="4" visible="no" active="yes"/>
<layer number="36" name="bGlue" color="7" fill="5" visible="no" active="yes"/>
<layer number="37" name="tTest" color="7" fill="1" visible="no" active="yes"/>
<layer number="38" name="bTest" color="7" fill="1" visible="no" active="yes"/>
<layer number="39" name="tKeepout" color="4" fill="11" visible="no" active="yes"/>
<layer number="40" name="bKeepout" color="1" fill="11" visible="no" active="yes"/>
<layer number="41" name="tRestrict" color="4" fill="10" visible="no" active="yes"/>
<layer number="42" name="bRestrict" color="1" fill="10" visible="no" active="yes"/>
<layer number="43" name="vRestrict" color="2" fill="10" visible="no" active="yes"/>
<layer number="44" name="Drills" color="7" fill="1" visible="no" active="yes"/>
<layer number="45" name="Holes" color="7" fill="1" visible="no" active="yes"/>
<layer number="46" name="Milling" color="3" fill="1" visible="no" active="yes"/>
<layer number="47" name="Measures" color="7" fill="1" visible="no" active="yes"/>
<layer number="48" name="Document" color="7" fill="1" visible="no" active="yes"/>
<layer number="49" name="Reference" color="7" fill="1" visible="no" active="yes"/>
<layer number="50" name="dxf" color="7" fill="1" visible="no" active="yes"/>
<layer number="51" name="tDocu" color="7" fill="1" visible="no" active="yes"/>
<layer number="52" name="bDocu" color="7" fill="1" visible="no" active="yes"/>
<layer number="53" name="tGND_GNDA" color="7" fill="9" visible="no" active="no"/>
<layer number="54" name="bGND_GNDA" color="1" fill="9" visible="no" active="no"/>
<layer number="56" name="wert" color="7" fill="1" visible="no" active="no"/>
<layer number="91" name="Nets" color="2" fill="1" visible="yes" active="yes"/>
<layer number="92" name="Busses" color="1" fill="1" visible="yes" active="yes"/>
<layer number="93" name="Pins" color="2" fill="1" visible="yes" active="yes"/>
<layer number="94" name="Symbols" color="4" fill="1" visible="yes" active="yes"/>
<layer number="95" name="Names" color="7" fill="1" visible="yes" active="yes"/>
<layer number="96" name="Values" color="7" fill="1" visible="yes" active="yes"/>
<layer number="97" name="Info" color="7" fill="1" visible="yes" active="yes"/>
<layer number="98" name="Guide" color="6" fill="1" visible="yes" active="yes"/>
<layer number="100" name="NonViaHole" color="14" fill="1" visible="no" active="yes"/>
<layer number="101" name="PlacementGuide" color="7" fill="1" visible="no" active="yes"/>
<layer number="102" name="Vscore" color="7" fill="1" visible="no" active="yes"/>
<layer number="103" name="tMap" color="7" fill="1" visible="no" active="yes"/>
<layer number="104" name="Name" color="16" fill="1" visible="no" active="yes"/>
<layer number="105" name="tPlate" color="7" fill="1" visible="no" active="yes"/>
<layer number="106" name="bPlate" color="7" fill="1" visible="no" active="yes"/>
<layer number="107" name="Crop" color="7" fill="1" visible="no" active="yes"/>
<layer number="108" name="tplace-old" color="10" fill="1" visible="no" active="yes"/>
<layer number="109" name="ref-old" color="11" fill="1" visible="no" active="yes"/>
<layer number="116" name="Patch_BOT" color="9" fill="4" visible="no" active="yes"/>
<layer number="121" name="_tsilk" color="7" fill="1" visible="no" active="yes"/>
<layer number="122" name="_bsilk" color="7" fill="1" visible="no" active="yes"/>
<layer number="125" name="_tNames" color="7" fill="1" visible="no" active="yes"/>
<layer number="144" name="Drill_legend" color="7" fill="1" visible="no" active="yes"/>
<layer number="151" name="HeatSink" color="7" fill="1" visible="no" active="yes"/>
<layer number="199" name="Contour" color="7" fill="1" visible="no" active="yes"/>
<layer number="200" name="200bmp" color="1" fill="10" visible="no" active="yes"/>
<layer number="201" name="201bmp" color="2" fill="10" visible="no" active="yes"/>
<layer number="202" name="202bmp" color="3" fill="10" visible="no" active="yes"/>
<layer number="203" name="203bmp" color="4" fill="10" visible="no" active="yes"/>
<layer number="204" name="204bmp" color="5" fill="10" visible="no" active="yes"/>
<layer number="205" name="205bmp" color="6" fill="10" visible="no" active="yes"/>
<layer number="206" name="206bmp" color="7" fill="10" visible="no" active="yes"/>
<layer number="207" name="207bmp" color="8" fill="10" visible="no" active="yes"/>
<layer number="208" name="208bmp" color="9" fill="10" visible="no" active="yes"/>
<layer number="209" name="209bmp" color="7" fill="1" visible="no" active="yes"/>
<layer number="210" name="210bmp" color="7" fill="1" visible="no" active="yes"/>
<layer number="211" name="211bmp" color="7" fill="1" visible="no" active="yes"/>
<layer number="212" name="212bmp" color="7" fill="1" visible="no" active="yes"/>
<layer number="213" name="213bmp" color="7" fill="1" visible="no" active="yes"/>
<layer number="214" name="214bmp" color="7" fill="1" visible="no" active="yes"/>
<layer number="215" name="215bmp" color="7" fill="1" visible="no" active="yes"/>
<layer number="216" name="216bmp" color="7" fill="1" visible="no" active="yes"/>
<layer number="217" name="217bmp" color="18" fill="1" visible="no" active="no"/>
<layer number="218" name="218bmp" color="19" fill="1" visible="no" active="no"/>
<layer number="219" name="219bmp" color="20" fill="1" visible="no" active="no"/>
<layer number="220" name="220bmp" color="21" fill="1" visible="no" active="no"/>
<layer number="221" name="221bmp" color="22" fill="1" visible="no" active="no"/>
<layer number="222" name="222bmp" color="23" fill="1" visible="no" active="no"/>
<layer number="223" name="223bmp" color="24" fill="1" visible="no" active="no"/>
<layer number="224" name="224bmp" color="25" fill="1" visible="no" active="no"/>
<layer number="231" name="Eagle3D_PG1" color="7" fill="1" visible="no" active="yes"/>
<layer number="232" name="Eagle3D_PG2" color="7" fill="1" visible="no" active="yes"/>
<layer number="233" name="Eagle3D_PG3" color="7" fill="1" visible="no" active="yes"/>
<layer number="250" name="Descript" color="7" fill="1" visible="no" active="yes"/>
<layer number="251" name="SMDround" color="7" fill="1" visible="no" active="yes"/>
<layer number="254" name="OrgLBR" color="7" fill="1" visible="no" active="yes"/>
</layers>
<library>
<description>&lt;b&gt;Common Voltage Regulators&lt;/b&gt;
&lt;p&gt;Created by Michael Shimniok &lt;a href="http://www.bot-thoughts.com/"&gt;www.bot-thoughts.com&lt;/a&gt;&lt;/b&gt;</description>
<packages>
<package name="SOT23-6">
<description>&lt;B&gt;SOT23-6 package&lt;/B&gt;

&lt;P&gt;This is the DBV6 package from Texas Instruments. It differs from the one in the Eagle libraries (there are two versions in ref-packages.lbr) in that the pad dimensions are 0.5mm x 1.4mm, as in the TI recommendation.
&lt;P&gt;The pin spacing is 0.95mm, and the package body has nominal dimensions 2.9mm long by 1.6mm wide.</description>
<wire x1="1.422" y1="-0.781" x2="-1.423" y2="-0.781" width="0.1524" layer="51"/>
<wire x1="-1.423" y1="-0.781" x2="-1.423" y2="0.781" width="0.2032" layer="21"/>
<wire x1="-1.423" y1="0.781" x2="1.422" y2="0.781" width="0.1524" layer="51"/>
<wire x1="1.422" y1="0.781" x2="1.422" y2="-0.781" width="0.2032" layer="21"/>
<wire x1="-1.4" y1="0" x2="-0.5" y2="0" width="0.2032" layer="21"/>
<wire x1="-0.5" y1="0" x2="-0.5" y2="-0.7" width="0.2032" layer="21"/>
<circle x="-1.0738" y="-0.4492" radius="0.1" width="0" layer="51"/>
<smd name="1" x="-0.95" y="-1.1" dx="0.5" dy="1.4" layer="1"/>
<smd name="2" x="0" y="-1.1" dx="0.5" dy="1.4" layer="1"/>
<smd name="3" x="0.95" y="-1.1" dx="0.5" dy="1.4" layer="1"/>
<smd name="4" x="0.95" y="1.1" dx="0.5" dy="1.4" layer="1"/>
<smd name="5" x="0" y="1.1" dx="0.5" dy="1.4" layer="1"/>
<smd name="6" x="-0.95" y="1.1" dx="0.5" dy="1.4" layer="1"/>
<text x="-1.524" y="-3.302" size="1.27" layer="27" font="vector" ratio="16">&gt;VALUE</text>
<text x="-1.524" y="2.286" size="1.27" layer="25" font="vector" ratio="16">&gt;NAME</text>
<rectangle x1="-1.2" y1="-1.4" x2="-0.7" y2="-0.8" layer="51"/>
<rectangle x1="-0.25" y1="-1.4" x2="0.25" y2="-0.8" layer="51"/>
<rectangle x1="0.7" y1="-1.4" x2="1.2" y2="-0.8" layer="51"/>
<rectangle x1="0.7" y1="0.8" x2="1.2" y2="1.4" layer="51"/>
<rectangle x1="-1.2" y1="0.8" x2="-0.7" y2="1.4" layer="51"/>
<rectangle x1="-0.25" y1="0.8" x2="0.25" y2="1.4" layer="51"/>
</package>
<package name="TO263-5">
<description>&lt;b&gt;TO-263&lt;/b&gt;</description>
<wire x1="5.094" y1="7.165" x2="5.094" y2="-2.88" width="0.2032" layer="51"/>
<wire x1="5.094" y1="-2.88" x2="-5.094" y2="-2.88" width="0.2032" layer="21"/>
<wire x1="-5.094" y1="-2.88" x2="-5.094" y2="7.165" width="0.2032" layer="51"/>
<wire x1="-5.094" y1="7.165" x2="5.094" y2="7.165" width="0.2032" layer="51"/>
<wire x1="-5.105" y1="7.267" x2="-5.105" y2="7.678" width="0.2032" layer="51"/>
<wire x1="-5.105" y1="7.678" x2="-3.378" y2="8.135" width="0.2032" layer="51"/>
<wire x1="-3.378" y1="8.135" x2="3.378" y2="8.135" width="0.2032" layer="51"/>
<wire x1="3.378" y1="8.135" x2="5.105" y2="7.678" width="0.2032" layer="51"/>
<wire x1="5.105" y1="7.678" x2="5.105" y2="7.267" width="0.2032" layer="51"/>
<wire x1="5.105" y1="7.267" x2="-5.105" y2="7.267" width="0.2032" layer="51"/>
<smd name="6" x="0" y="2.54" dx="10.8" dy="10.41" layer="1"/>
<smd name="1" x="-3.4036" y="-5.7912" dx="1.0668" dy="2.159" layer="1"/>
<smd name="2" x="-1.7018" y="-5.7912" dx="1.0668" dy="2.159" layer="1"/>
<smd name="3" x="0" y="-5.7912" dx="1.0668" dy="2.159" layer="1"/>
<smd name="4" x="1.7018" y="-5.7912" dx="1.0668" dy="2.159" layer="1"/>
<smd name="5" x="3.4036" y="-5.7912" dx="1.0668" dy="2.159" layer="1"/>
<text x="-5.588" y="-5.588" size="1.27" layer="25" rot="R90">&gt;NAME</text>
<text x="6.858" y="-5.588" size="1.27" layer="27" rot="R90">&gt;VALUE</text>
<rectangle x1="-3.8862" y1="-6.604" x2="-2.921" y2="-4.445" layer="51"/>
<rectangle x1="-3.8862" y1="-4.4704" x2="-2.921" y2="-2.794" layer="21"/>
<rectangle x1="-2.1844" y1="-6.604" x2="-1.2192" y2="-4.445" layer="51"/>
<rectangle x1="-0.4826" y1="-6.604" x2="0.4826" y2="-4.445" layer="51"/>
<rectangle x1="1.2192" y1="-6.604" x2="2.1844" y2="-4.445" layer="51"/>
<rectangle x1="2.921" y1="-6.604" x2="3.8862" y2="-4.445" layer="51"/>
<rectangle x1="-2.1844" y1="-4.4704" x2="-1.2192" y2="-2.794" layer="21"/>
<rectangle x1="-0.4826" y1="-4.4704" x2="0.4826" y2="-2.794" layer="21"/>
<rectangle x1="1.2192" y1="-4.4704" x2="2.1844" y2="-2.794" layer="21"/>
<rectangle x1="2.921" y1="-4.4704" x2="3.8862" y2="-2.794" layer="21"/>
<polygon width="0.2032" layer="51">
<vertex x="-5.1054" y="7.267"/>
<vertex x="-5.1054" y="7.6782"/>
<vertex x="-3.3782" y="8.1354"/>
<vertex x="3.3782" y="8.1354"/>
<vertex x="5.1054" y="7.6782"/>
<vertex x="5.1054" y="7.267"/>
</polygon>
</package>
<package name="TO220-5">
<description>&lt;b&gt;TO220-5&lt;/b&gt;</description>
<wire x1="-1.87" y1="-0.2" x2="-1.87" y2="-0.3" width="0.0508" layer="51"/>
<wire x1="-1.87" y1="-0.4" x2="-1.87" y2="-0.5" width="0.0508" layer="51"/>
<wire x1="-1.87" y1="-0.6" x2="-1.87" y2="-0.7" width="0.0508" layer="51"/>
<wire x1="-1.87" y1="-1" x2="-1.87" y2="-1.17" width="0.0508" layer="51"/>
<wire x1="1.87" y1="-1.17" x2="1.87" y2="-1" width="0.0508" layer="51"/>
<wire x1="1.87" y1="-0.9" x2="1.87" y2="-0.8" width="0.0508" layer="51"/>
<wire x1="1.87" y1="-0.7" x2="1.87" y2="-0.6" width="0.0508" layer="51"/>
<wire x1="1.87" y1="-0.5" x2="1.87" y2="-0.4" width="0.0508" layer="51"/>
<wire x1="1.87" y1="-0.3" x2="1.87" y2="-0.2" width="0.0508" layer="51"/>
<wire x1="-5" y1="-0.1" x2="-5" y2="-1.2" width="0.2032" layer="21"/>
<wire x1="-4.9" y1="-1.2" x2="-4.9" y2="-3.6" width="0.2032" layer="51"/>
<wire x1="-4.9" y1="-3.6" x2="-4.5" y2="-4.5" width="0.2032" layer="51"/>
<wire x1="-4.5" y1="-4.5" x2="4.5" y2="-4.5" width="0.2032" layer="51"/>
<wire x1="4.5" y1="-4.5" x2="4.9" y2="-3.6" width="0.2032" layer="51"/>
<wire x1="4.9" y1="-3.6" x2="4.9" y2="-1.2" width="0.2032" layer="51"/>
<wire x1="5" y1="-1.2" x2="5" y2="-0.1" width="0.2032" layer="21"/>
<wire x1="5" y1="-0.1" x2="-5" y2="-0.1" width="0.2032" layer="21"/>
<wire x1="-5" y1="-1.2" x2="5" y2="-1.2" width="0.2032" layer="21"/>
<wire x1="-1.87" y1="-0.8" x2="-1.87" y2="-0.9" width="0.0508" layer="51"/>
<wire x1="-4.9" y1="-3.6" x2="4.9" y2="-3.6" width="0.2032" layer="51"/>
<pad name="2" x="-1.7" y="-4.5" drill="0.9" shape="long" rot="R90"/>
<pad name="4" x="1.7" y="-4.5" drill="0.9" shape="long" rot="R90"/>
<pad name="1" x="-3.4" y="-8.4" drill="0.9" shape="long" rot="R90"/>
<pad name="3" x="0" y="-8.4" drill="0.9" shape="long" rot="R90"/>
<pad name="5" x="3.4" y="-8.4" drill="0.9" shape="long" rot="R90"/>
<text x="-5.08" y="-8.382" size="1.27" layer="25" rot="R90">&gt;NAME</text>
<text x="6.35" y="-8.382" size="1.27" layer="27" rot="R90">&gt;VALUE</text>
<rectangle x1="-3.8" y1="-8.6" x2="-3" y2="-7.5" layer="51"/>
<rectangle x1="-0.4" y1="-8.6" x2="0.4" y2="-7.5" layer="51"/>
<rectangle x1="3" y1="-8.6" x2="3.8" y2="-7.5" layer="51"/>
<rectangle x1="-3.8" y1="-7.5" x2="-3" y2="-4.5" layer="51"/>
<rectangle x1="-0.4" y1="-7.5" x2="0.4" y2="-4.5" layer="51"/>
<rectangle x1="3" y1="-7.5" x2="3.8" y2="-4.5" layer="51"/>
<rectangle x1="-2.1" y1="-4.7" x2="-1.3" y2="-4.5" layer="51"/>
<rectangle x1="1.3" y1="-4.7" x2="2.1" y2="-4.5" layer="51"/>
</package>
<package name="SO08">
<description>&lt;b&gt;SMALL OUTLINE INTEGRATED CIRCUIT&lt;/b&gt;&lt;p&gt;
body 3.9 mm/JEDEC MS-012AA</description>
<wire x1="-2.9" y1="3.9" x2="2.9" y2="3.9" width="0.1998" layer="39"/>
<wire x1="2.9" y1="3.9" x2="2.9" y2="-3.9" width="0.1998" layer="39"/>
<wire x1="2.9" y1="-3.9" x2="-2.9" y2="-3.9" width="0.1998" layer="39"/>
<wire x1="-2.9" y1="-3.9" x2="-2.9" y2="3.9" width="0.1998" layer="39"/>
<wire x1="2.4" y1="1.9" x2="2.4" y2="-1.9" width="0.1778" layer="21"/>
<wire x1="2.4" y1="-1.9" x2="-2.4" y2="-1.9" width="0.1778" layer="51"/>
<wire x1="-2.4" y1="-1.9" x2="-2.4" y2="1.9" width="0.1778" layer="21"/>
<wire x1="-2.4" y1="1.9" x2="2.4" y2="1.9" width="0.1778" layer="51"/>
<wire x1="2.4" y1="-1.4" x2="-2.4" y2="-1.4" width="0.0508" layer="51"/>
<circle x="-1.905" y="-0.9525" radius="0.2245" width="0" layer="21"/>
<smd name="2" x="-0.635" y="-2.6" dx="0.6" dy="2.2" layer="1"/>
<smd name="7" x="-0.635" y="2.6" dx="0.6" dy="2.2" layer="1"/>
<smd name="1" x="-1.905" y="-2.6" dx="0.6" dy="2.2" layer="1"/>
<smd name="3" x="0.635" y="-2.6" dx="0.6" dy="2.2" layer="1"/>
<smd name="4" x="1.905" y="-2.6" dx="0.6" dy="2.2" layer="1"/>
<smd name="8" x="-1.905" y="2.6" dx="0.6" dy="2.2" layer="1"/>
<smd name="6" x="0.635" y="2.6" dx="0.6" dy="2.2" layer="1"/>
<smd name="5" x="1.905" y="2.6" dx="0.6" dy="2.2" layer="1"/>
<text x="-3.175" y="-1.905" size="1.27" layer="25" ratio="10" rot="R90">&gt;NAME</text>
<text x="4.445" y="-1.905" size="1.27" layer="27" ratio="10" rot="R90">&gt;VALUE</text>
<rectangle x1="-2.1501" y1="-3.1001" x2="-1.6599" y2="-2" layer="51"/>
<rectangle x1="-0.8801" y1="-3.1001" x2="-0.3899" y2="-2" layer="51"/>
<rectangle x1="0.3899" y1="-3.1001" x2="0.8801" y2="-2" layer="51"/>
<rectangle x1="1.6599" y1="-3.1001" x2="2.1501" y2="-2" layer="51"/>
<rectangle x1="1.6599" y1="2" x2="2.1501" y2="3.1001" layer="51"/>
<rectangle x1="0.3899" y1="2" x2="0.8801" y2="3.1001" layer="51"/>
<rectangle x1="-0.8801" y1="2" x2="-0.3899" y2="3.1001" layer="51"/>
<rectangle x1="-2.1501" y1="2" x2="-1.6599" y2="3.1001" layer="51"/>
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
<smd name="1" x="-0.95" y="-1.3001" dx="0.69" dy="0.99" layer="1"/>
<smd name="2" x="0" y="-1.3001" dx="0.69" dy="0.99" layer="1"/>
<smd name="3" x="0.95" y="-1.3001" dx="0.69" dy="0.99" layer="1"/>
<smd name="4" x="0.95" y="1.3001" dx="0.69" dy="0.99" layer="1"/>
<smd name="5" x="-0.95" y="1.3001" dx="0.69" dy="0.99" layer="1"/>
<text x="-1.6095" y="-1.1525" size="0.4064" layer="27" rot="R90">&gt;VALUE</text>
<wire x1="1.43" y1="0.8" x2="1.43" y2="-0.8" width="0.127" layer="21"/>
<wire x1="1.43" y1="-0.8" x2="-1.41" y2="-0.8" width="0.127" layer="51"/>
<wire x1="-1.41" y1="-0.8" x2="-1.41" y2="0.8" width="0.127" layer="21"/>
<wire x1="-1.41" y1="0.8" x2="1.43" y2="0.8" width="0.127" layer="51"/>
<text x="-0.495" y="-0.395" size="0.8128" layer="25">&gt;NAME</text>
<rectangle x1="-1.1" y1="0.8" x2="-0.77" y2="1.43" layer="51"/>
<rectangle x1="0.8" y1="0.8" x2="1.13" y2="1.42" layer="51"/>
<rectangle x1="-1.1" y1="-1.42" x2="-0.77" y2="-0.8" layer="51"/>
<rectangle x1="-0.15" y1="-1.42" x2="0.18" y2="-0.8" layer="51"/>
<rectangle x1="0.8" y1="-1.42" x2="1.13" y2="-0.8" layer="51"/>
<rectangle x1="-1.365" y1="-0.75" x2="-0.615" y2="0" layer="21"/>
</package>
<package name="DPAK">
<description>&lt;B&gt;D-PAK SMT Package&lt;/B&gt;
&lt;P&gt;Similar to TO-252, but pad size and spacing as suggested by ST Microelectronics LD1117 devices&lt;/B&gt;</description>
<wire x1="3.7766" y1="3.8354" x2="3.777" y2="-2.159" width="0.2032" layer="21"/>
<wire x1="3.777" y1="-2.159" x2="-3.777" y2="-2.159" width="0.2032" layer="21"/>
<wire x1="-3.777" y1="-2.159" x2="-3.7766" y2="3.8354" width="0.2032" layer="21"/>
<wire x1="-3.277" y1="3.835" x2="3.2774" y2="3.8346" width="0.2032" layer="51"/>
<wire x1="-3.973" y1="5.983" x2="4.073" y2="5.983" width="0.0508" layer="39"/>
<wire x1="4.073" y1="-6.783" x2="-3.973" y2="-6.783" width="0.0508" layer="39"/>
<wire x1="-3.973" y1="-6.783" x2="-3.973" y2="5.983" width="0.0508" layer="39"/>
<wire x1="4.073" y1="5.983" x2="4.073" y2="-6.783" width="0.0508" layer="39"/>
<wire x1="-2.5654" y1="3.937" x2="-2.5654" y2="4.6482" width="0.2032" layer="51"/>
<wire x1="-2.5654" y1="4.6482" x2="-2.1082" y2="5.1054" width="0.2032" layer="51"/>
<wire x1="-2.1082" y1="5.1054" x2="2.1082" y2="5.1054" width="0.2032" layer="51"/>
<wire x1="2.1082" y1="5.1054" x2="2.5654" y2="4.6482" width="0.2032" layer="51"/>
<wire x1="2.5654" y1="4.6482" x2="2.5654" y2="3.937" width="0.2032" layer="51"/>
<wire x1="2.5654" y1="3.937" x2="-2.5654" y2="3.937" width="0.2032" layer="51"/>
<smd name="4" x="0" y="1.86" dx="6.7" dy="6.7" layer="1"/>
<smd name="1" x="-2.3" y="-4.8" dx="1.6" dy="3" layer="1"/>
<smd name="3" x="2.3" y="-4.8" dx="1.6" dy="3" layer="1"/>
<text x="-3.24" y="6.21" size="1.27" layer="25" font="vector" ratio="16">&gt;NAME</text>
<text x="-4.32" y="-2.44" size="1.27" layer="27" font="vector" ratio="16" rot="R90">&gt;VALUE</text>
<rectangle x1="-2.7178" y1="-5.1562" x2="-1.8542" y2="-2.2606" layer="51"/>
<rectangle x1="1.8542" y1="-5.1562" x2="2.7178" y2="-2.2606" layer="51"/>
<rectangle x1="-0.4318" y1="-3.0226" x2="0.4318" y2="-2.2606" layer="21"/>
<polygon width="0.1998" layer="51">
<vertex x="-2.5654" y="3.937"/>
<vertex x="-2.5654" y="4.6482"/>
<vertex x="-2.1082" y="5.1054"/>
<vertex x="2.1082" y="5.1054"/>
<vertex x="2.5654" y="4.6482"/>
<vertex x="2.5654" y="3.937"/>
</polygon>
</package>
<package name="SOT-223-3">
<wire x1="3.2766" y1="1.651" x2="3.2766" y2="-1.651" width="0.2032" layer="21"/>
<wire x1="3.2766" y1="-1.651" x2="-3.2766" y2="-1.651" width="0.2032" layer="21"/>
<wire x1="-3.2766" y1="-1.651" x2="-3.2766" y2="1.651" width="0.2032" layer="21"/>
<wire x1="-3.2766" y1="1.651" x2="3.2766" y2="1.651" width="0.2032" layer="21"/>
<smd name="1" x="-2.3114" y="-3.0988" dx="1.2192" dy="2.2352" layer="1"/>
<smd name="2" x="0" y="-3.0988" dx="1.2192" dy="2.2352" layer="1"/>
<smd name="3" x="2.3114" y="-3.0988" dx="1.2192" dy="2.2352" layer="1"/>
<smd name="4" x="0" y="3.099" dx="3.6" dy="2.2" layer="1"/>
<text x="-2.7305" y="0.1905" size="1.016" layer="25">&gt;NAME</text>
<text x="-2.7305" y="-1.2065" size="1.016" layer="27">&gt;VALUE</text>
<rectangle x1="-1.6002" y1="1.8034" x2="1.6002" y2="3.6576" layer="51"/>
<rectangle x1="-0.4318" y1="-3.6576" x2="0.4318" y2="-1.8034" layer="51"/>
<rectangle x1="-2.7432" y1="-3.6576" x2="-1.8796" y2="-1.8034" layer="51"/>
<rectangle x1="1.8796" y1="-3.6576" x2="2.7432" y2="-1.8034" layer="51"/>
<rectangle x1="-1.6002" y1="1.8034" x2="1.6002" y2="3.6576" layer="51"/>
<rectangle x1="-0.4318" y1="-3.6576" x2="0.4318" y2="-1.8034" layer="51"/>
<rectangle x1="-2.7432" y1="-3.6576" x2="-1.8796" y2="-1.8034" layer="51"/>
<rectangle x1="1.8796" y1="-3.6576" x2="2.7432" y2="-1.8034" layer="51"/>
</package>
<package name="TO220L1">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
<wire x1="-5.207" y1="-1.27" x2="5.207" y2="-1.27" width="0.1524" layer="21"/>
<wire x1="5.207" y1="14.605" x2="-5.207" y2="14.605" width="0.1524" layer="21"/>
<wire x1="5.207" y1="-1.27" x2="5.207" y2="11.176" width="0.1524" layer="21"/>
<wire x1="5.207" y1="11.176" x2="4.318" y2="11.176" width="0.1524" layer="21"/>
<wire x1="4.318" y1="11.176" x2="4.318" y2="12.7" width="0.1524" layer="21"/>
<wire x1="4.318" y1="12.7" x2="5.207" y2="12.7" width="0.1524" layer="21"/>
<wire x1="5.207" y1="12.7" x2="5.207" y2="14.605" width="0.1524" layer="21"/>
<wire x1="-5.207" y1="-1.27" x2="-5.207" y2="11.176" width="0.1524" layer="21"/>
<wire x1="-5.207" y1="11.176" x2="-4.318" y2="11.176" width="0.1524" layer="21"/>
<wire x1="-4.318" y1="11.176" x2="-4.318" y2="12.7" width="0.1524" layer="21"/>
<wire x1="-4.318" y1="12.7" x2="-5.207" y2="12.7" width="0.1524" layer="21"/>
<wire x1="-5.207" y1="12.7" x2="-5.207" y2="14.605" width="0.1524" layer="21"/>
<wire x1="-4.572" y1="-0.635" x2="4.572" y2="-0.635" width="0.0508" layer="21"/>
<wire x1="4.572" y1="7.62" x2="4.572" y2="-0.635" width="0.0508" layer="21"/>
<wire x1="4.572" y1="7.62" x2="-4.572" y2="7.62" width="0.0508" layer="21"/>
<wire x1="-4.572" y1="-0.635" x2="-4.572" y2="7.62" width="0.0508" layer="21"/>
<circle x="0" y="11.176" radius="1.8034" width="0.1524" layer="21"/>
<circle x="0" y="11.176" radius="4.191" width="0" layer="42"/>
<circle x="0" y="11.176" radius="4.191" width="0" layer="43"/>
<pad name="1" x="-2.54" y="-3.81" drill="1.016" shape="long" rot="R90"/>
<pad name="2" x="0" y="-3.81" drill="1.016" shape="long" rot="R90"/>
<pad name="3" x="2.54" y="-3.81" drill="1.016" shape="long" rot="R90"/>
<text x="-3.81" y="5.08" size="1.778" layer="25" ratio="10">&gt;NAME</text>
<text x="-3.937" y="2.54" size="1.778" layer="27" ratio="10">&gt;VALUE</text>
<text x="-4.445" y="7.874" size="0.9906" layer="21" ratio="10">A15,2mm</text>
<text x="-3.048" y="0" size="1.27" layer="51" ratio="10">1</text>
<text x="-0.508" y="0" size="1.27" layer="51" ratio="10">2</text>
<text x="2.032" y="0" size="1.27" layer="51" ratio="10">3</text>
<rectangle x1="1.905" y1="-2.159" x2="3.175" y2="-1.27" layer="21"/>
<rectangle x1="1.905" y1="-3.81" x2="3.175" y2="-2.159" layer="51"/>
<rectangle x1="-0.635" y1="-2.159" x2="0.635" y2="-1.27" layer="21"/>
<rectangle x1="-3.175" y1="-2.159" x2="-1.905" y2="-1.27" layer="21"/>
<rectangle x1="-0.635" y1="-3.81" x2="0.635" y2="-2.159" layer="51"/>
<rectangle x1="-3.175" y1="-3.81" x2="-1.905" y2="-2.159" layer="51"/>
<hole x="0" y="11.176" drill="3.302"/>
<pad name="4" x="0" y="11.176" drill="3.2"/>
</package>
<package name="TO220S">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
<wire x1="4.826" y1="-4.318" x2="5.08" y2="-4.064" width="0.1524" layer="21"/>
<wire x1="4.826" y1="-4.318" x2="-4.826" y2="-4.318" width="0.1524" layer="21"/>
<wire x1="-5.08" y1="-4.064" x2="-4.826" y2="-4.318" width="0.1524" layer="21"/>
<wire x1="5.08" y1="-1.143" x2="5.08" y2="-4.064" width="0.1524" layer="21"/>
<wire x1="-5.08" y1="-4.064" x2="-5.08" y2="-1.143" width="0.1524" layer="21"/>
<circle x="-4.6228" y="-3.7084" radius="0.254" width="0" layer="21"/>
<pad name="1" x="-2.54" y="-2.54" drill="1.016" shape="long" rot="R90"/>
<pad name="2" x="0" y="-2.54" drill="1.016" shape="long" rot="R90"/>
<pad name="3" x="2.54" y="-2.54" drill="1.016" shape="long" rot="R90"/>
<text x="-5.08" y="-5.9182" size="1.27" layer="25" ratio="10">&gt;NAME</text>
<text x="-5.08" y="-7.62" size="1.27" layer="27" ratio="10">&gt;VALUE</text>
<text x="-3.175" y="-3.81" size="1.27" layer="51" ratio="10">1</text>
<text x="-0.635" y="-3.81" size="1.27" layer="51" ratio="10">2</text>
<text x="1.905" y="-3.81" size="1.27" layer="51" ratio="10">3</text>
<rectangle x1="-5.334" y1="-1.27" x2="-3.429" y2="0" layer="21"/>
<rectangle x1="-3.429" y1="-0.762" x2="-1.651" y2="0" layer="21"/>
<rectangle x1="-1.651" y1="-1.27" x2="-0.889" y2="0" layer="21"/>
<rectangle x1="-0.889" y1="-0.762" x2="0.889" y2="0" layer="21"/>
<rectangle x1="0.889" y1="-1.27" x2="1.651" y2="0" layer="21"/>
<rectangle x1="1.651" y1="-0.762" x2="3.429" y2="0" layer="21"/>
<rectangle x1="3.429" y1="-1.27" x2="5.334" y2="0" layer="21"/>
<rectangle x1="-3.429" y1="-1.27" x2="-1.651" y2="-0.762" layer="51"/>
<rectangle x1="-0.889" y1="-1.27" x2="0.889" y2="-0.762" layer="51"/>
<rectangle x1="1.651" y1="-1.27" x2="3.429" y2="-0.762" layer="51"/>
</package>
<package name="TO263-3">
<wire x1="5.094" y1="5.895" x2="5.094" y2="-4.15" width="0.2032" layer="51"/>
<wire x1="5.094" y1="-4.15" x2="-5.094" y2="-4.15" width="0.2032" layer="21"/>
<wire x1="-5.094" y1="-4.15" x2="-5.094" y2="5.895" width="0.2032" layer="51"/>
<wire x1="-5.094" y1="5.895" x2="5.094" y2="5.895" width="0.2032" layer="51"/>
<wire x1="-5.105" y1="5.997" x2="-5.105" y2="6.408" width="0.2032" layer="51"/>
<wire x1="-5.105" y1="6.408" x2="-3.378" y2="6.865" width="0.2032" layer="51"/>
<wire x1="-3.378" y1="6.865" x2="3.378" y2="6.865" width="0.2032" layer="51"/>
<wire x1="3.378" y1="6.865" x2="5.105" y2="6.408" width="0.2032" layer="51"/>
<wire x1="5.105" y1="6.408" x2="5.105" y2="5.997" width="0.2032" layer="51"/>
<wire x1="5.105" y1="5.997" x2="-5.105" y2="5.997" width="0.2032" layer="51"/>
<smd name="4" x="0" y="3.81" dx="10.795" dy="7.493" layer="1"/>
<smd name="1" x="-2.54" y="-7.0612" dx="1.0668" dy="2.159" layer="1"/>
<smd name="2" x="0" y="-7.0612" dx="1.0668" dy="2.159" layer="1"/>
<smd name="3" x="2.54" y="-7.0612" dx="1.0668" dy="2.159" layer="1"/>
<text x="-5.588" y="-6.858" size="1.27" layer="25" rot="R90">&gt;NAME</text>
<text x="6.858" y="-6.858" size="1.27" layer="27" rot="R90">&gt;VALUE</text>
<rectangle x1="2.159" y1="-7.874" x2="2.921" y2="-5.715" layer="51"/>
<rectangle x1="-2.921" y1="-5.7404" x2="-2.159" y2="-4.064" layer="21"/>
<rectangle x1="-0.381" y1="-7.874" x2="0.381" y2="-5.715" layer="51"/>
<rectangle x1="-0.381" y1="-5.7404" x2="0.381" y2="-4.064" layer="21"/>
<polygon width="0.2032" layer="51">
<vertex x="-5.1054" y="5.997"/>
<vertex x="-5.1054" y="6.4082"/>
<vertex x="-3.3782" y="6.8654"/>
<vertex x="3.3782" y="6.8654"/>
<vertex x="5.1054" y="6.4082"/>
<vertex x="5.1054" y="5.997"/>
</polygon>
<rectangle x1="-2.921" y1="-7.874" x2="-2.159" y2="-5.715" layer="51"/>
<rectangle x1="2.159" y1="-5.7404" x2="2.921" y2="-4.064" layer="21"/>
</package>
<package name="D2PACK">
<description>&lt;b&gt;D2PACK&lt;/b&gt;&lt;p&gt;
Source: INTERNATIONAL RECTIFIER, irg4bc15ud-s.pdf</description>
<wire x1="-5.1308" y1="-4.0894" x2="5.1308" y2="-4.0894" width="0.254" layer="21"/>
<wire x1="5.1308" y1="-4.0894" x2="5.1308" y2="4.445" width="0.254" layer="51"/>
<wire x1="5.1308" y1="4.445" x2="3.1242" y2="5.8166" width="0.254" layer="51"/>
<wire x1="3.1242" y1="5.8166" x2="-3.3782" y2="5.8166" width="0.254" layer="51"/>
<wire x1="-3.3782" y1="5.8166" x2="-5.1308" y2="4.699" width="0.254" layer="51"/>
<wire x1="-5.1308" y1="4.699" x2="-5.1308" y2="4.445" width="0.254" layer="51"/>
<wire x1="-5.1308" y1="4.445" x2="-5.1308" y2="-4.0894" width="0.254" layer="51"/>
<wire x1="-5.1308" y1="4.445" x2="5.1308" y2="4.445" width="0.254" layer="51"/>
<wire x1="-5.1308" y1="-4.0894" x2="-5.1308" y2="-2.3114" width="0.254" layer="21"/>
<wire x1="5.1308" y1="-4.0894" x2="5.1308" y2="-2.3114" width="0.254" layer="21"/>
<smd name="1" x="-2.54" y="-8.89" dx="2.0828" dy="3.81" layer="1"/>
<smd name="3" x="2.54" y="-8.89" dx="2.0828" dy="3.81" layer="1"/>
<smd name="2" x="0" y="2.54" dx="11.43" dy="8.89" layer="1"/>
<text x="-5.588" y="7.239" size="1.27" layer="25">&gt;NAME</text>
<text x="-3.81" y="-3.429" size="1.27" layer="27">&gt;VALUE</text>
<rectangle x1="-3.0988" y1="-9.525" x2="-1.9812" y2="-8.1026" layer="51"/>
<rectangle x1="-3.2512" y1="-8.1534" x2="-1.8288" y2="-6.731" layer="51"/>
<rectangle x1="-3.2512" y1="-6.731" x2="-1.8288" y2="-4.2418" layer="21"/>
<rectangle x1="1.9812" y1="-9.525" x2="3.0988" y2="-8.1026" layer="51"/>
<rectangle x1="1.8288" y1="-8.1534" x2="3.2512" y2="-6.731" layer="51"/>
<rectangle x1="1.8288" y1="-6.731" x2="3.2512" y2="-4.2418" layer="21"/>
<rectangle x1="-0.7112" y1="-6.731" x2="0.7112" y2="-4.2418" layer="21"/>
</package>
<package name="D2PACK-3">
<wire x1="-5.1308" y1="-4.0894" x2="5.1308" y2="-4.0894" width="0.254" layer="21"/>
<wire x1="-5.1308" y1="-4.0894" x2="-5.1308" y2="-2.3114" width="0.254" layer="21"/>
<wire x1="5.1308" y1="-4.0894" x2="5.1308" y2="-2.3114" width="0.254" layer="21"/>
<smd name="1" x="-2.54" y="-8.89" dx="2.0828" dy="3.81" layer="1"/>
<smd name="2" x="0" y="-8.89" dx="2.0828" dy="3.81" layer="1"/>
<smd name="4" x="0" y="2.54" dx="11.43" dy="8.89" layer="1"/>
<text x="-5.588" y="7.239" size="1.27" layer="25">&gt;NAME</text>
<text x="-3.81" y="-3.429" size="1.27" layer="27">&gt;VALUE</text>
<rectangle x1="-3.2512" y1="-6.731" x2="-1.8288" y2="-4.2418" layer="21"/>
<rectangle x1="1.8288" y1="-6.731" x2="3.2512" y2="-4.2418" layer="21"/>
<rectangle x1="-0.7112" y1="-6.731" x2="0.7112" y2="-4.2418" layer="21"/>
<smd name="3" x="2.54" y="-8.89" dx="2.0828" dy="3.81" layer="1"/>
</package>
<package name="TO220BV">
<description>&lt;B&gt;TO220BV&lt;/B&gt; from transistor-power.lbr</description>
<wire x1="4.699" y1="-1.778" x2="4.953" y2="-1.524" width="0.1524" layer="21"/>
<wire x1="4.699" y1="-1.778" x2="-4.699" y2="-1.778" width="0.1524" layer="21"/>
<wire x1="-4.953" y1="-1.524" x2="-4.699" y2="-1.778" width="0.1524" layer="21"/>
<wire x1="5.08" y1="1.397" x2="4.953" y2="-1.524" width="0.1524" layer="21"/>
<wire x1="-4.953" y1="-1.524" x2="-5.08" y2="1.397" width="0.1524" layer="21"/>
<circle x="-4.4958" y="-1.1684" radius="0.254" width="0" layer="21"/>
<pad name="1" x="-2.54" y="0" drill="1.016" shape="long" rot="R90"/>
<pad name="2" x="0" y="0" drill="1.016" shape="long" rot="R90"/>
<pad name="3" x="2.54" y="0" drill="1.016" shape="long" rot="R90"/>
<text x="-5.08" y="-3.5052" size="1.27" layer="25" ratio="10">&gt;NAME</text>
<text x="-5.08" y="-5.08" size="1.27" layer="27" ratio="10">&gt;VALUE</text>
<rectangle x1="-5.334" y1="1.778" x2="5.334" y2="2.54" layer="21"/>
<rectangle x1="-5.334" y1="1.27" x2="-3.429" y2="1.778" layer="21"/>
<rectangle x1="-1.651" y1="1.27" x2="-0.889" y2="1.778" layer="21"/>
<rectangle x1="-3.429" y1="1.27" x2="-1.651" y2="1.778" layer="51"/>
<rectangle x1="0.889" y1="1.27" x2="1.651" y2="1.778" layer="21"/>
<rectangle x1="3.429" y1="1.27" x2="5.334" y2="1.778" layer="21"/>
<rectangle x1="-0.889" y1="1.27" x2="0.889" y2="1.778" layer="51"/>
<rectangle x1="1.651" y1="1.27" x2="3.429" y2="1.778" layer="51"/>
</package>
<package name="TO220BH">
<description>&lt;b&gt;TO220 Horizontal&lt;/b&gt;&lt;p&gt;
From transistor-power.lbr</description>
<wire x1="-5.207" y1="-1.27" x2="5.207" y2="-1.27" width="0.1524" layer="21"/>
<wire x1="5.207" y1="14.605" x2="-5.207" y2="14.605" width="0.1524" layer="21"/>
<wire x1="5.207" y1="-1.27" x2="5.207" y2="11.176" width="0.1524" layer="21"/>
<wire x1="5.207" y1="11.176" x2="4.318" y2="11.176" width="0.1524" layer="21"/>
<wire x1="4.318" y1="11.176" x2="4.318" y2="12.7" width="0.1524" layer="21"/>
<wire x1="4.318" y1="12.7" x2="5.207" y2="12.7" width="0.1524" layer="21"/>
<wire x1="5.207" y1="12.7" x2="5.207" y2="14.605" width="0.1524" layer="21"/>
<wire x1="-5.207" y1="-1.27" x2="-5.207" y2="11.176" width="0.1524" layer="21"/>
<wire x1="-5.207" y1="11.176" x2="-4.318" y2="11.176" width="0.1524" layer="21"/>
<wire x1="-4.318" y1="11.176" x2="-4.318" y2="12.7" width="0.1524" layer="21"/>
<wire x1="-4.318" y1="12.7" x2="-5.207" y2="12.7" width="0.1524" layer="21"/>
<wire x1="-5.207" y1="12.7" x2="-5.207" y2="14.605" width="0.1524" layer="21"/>
<wire x1="-4.572" y1="-0.635" x2="4.572" y2="-0.635" width="0.0508" layer="21"/>
<wire x1="4.572" y1="7.62" x2="4.572" y2="-0.635" width="0.0508" layer="21"/>
<wire x1="4.572" y1="7.62" x2="-4.572" y2="7.62" width="0.0508" layer="21"/>
<wire x1="-4.572" y1="-0.635" x2="-4.572" y2="7.62" width="0.0508" layer="21"/>
<circle x="0" y="11.176" radius="1.8034" width="0.1524" layer="21"/>
<circle x="0" y="11.176" radius="4.191" width="0" layer="42"/>
<circle x="0" y="11.176" radius="4.191" width="0" layer="43"/>
<pad name="1" x="-2.54" y="-6.35" drill="1.1176" shape="long" rot="R90"/>
<pad name="2" x="0" y="-6.35" drill="1.1176" shape="long" rot="R90"/>
<pad name="3" x="2.54" y="-6.35" drill="1.1176" shape="long" rot="R90"/>
<text x="-3.81" y="5.207" size="1.778" layer="25" font="vector" ratio="12">&gt;NAME</text>
<text x="-3.937" y="2.54" size="1.778" layer="27" font="vector" ratio="12">&gt;VALUE</text>
<text x="-4.445" y="7.874" size="1.016" layer="21" ratio="10">A17,5mm</text>
<rectangle x1="2.159" y1="-4.699" x2="2.921" y2="-4.064" layer="21"/>
<rectangle x1="-0.381" y1="-4.699" x2="0.381" y2="-4.064" layer="21"/>
<rectangle x1="-2.921" y1="-4.699" x2="-2.159" y2="-4.064" layer="21"/>
<rectangle x1="-3.175" y1="-4.064" x2="-1.905" y2="-1.27" layer="21"/>
<rectangle x1="-0.635" y1="-4.064" x2="0.635" y2="-1.27" layer="21"/>
<rectangle x1="1.905" y1="-4.064" x2="3.175" y2="-1.27" layer="21"/>
<rectangle x1="-2.921" y1="-6.604" x2="-2.159" y2="-4.699" layer="51"/>
<rectangle x1="-0.381" y1="-6.604" x2="0.381" y2="-4.699" layer="51"/>
<rectangle x1="2.159" y1="-6.604" x2="2.921" y2="-4.699" layer="51"/>
<hole x="0" y="11.176" drill="3.302"/>
</package>
</packages>
<symbols>
<symbol name="MIC5320">
<wire x1="-10.16" y1="10.16" x2="10.16" y2="10.16" width="0.254" layer="94"/>
<wire x1="10.16" y1="10.16" x2="10.16" y2="-10.16" width="0.254" layer="94"/>
<wire x1="10.16" y1="-10.16" x2="-10.16" y2="-10.16" width="0.254" layer="94"/>
<wire x1="-10.16" y1="-10.16" x2="-10.16" y2="10.16" width="0.254" layer="94"/>
<text x="-10.16" y="-13.97" size="1.778" layer="95">&gt;NAME</text>
<text x="-10.16" y="11.43" size="1.778" layer="95">&gt;VALUE</text>
<pin name="VIN" x="-15.24" y="7.62" visible="pin" length="middle" direction="sup"/>
<pin name="EN1" x="-15.24" y="2.54" visible="pin" length="middle" direction="in"/>
<pin name="EN2" x="-15.24" y="-2.54" visible="pin" length="middle" direction="in"/>
<pin name="GND" x="-15.24" y="-7.62" visible="pin" length="middle" direction="sup"/>
<pin name="VOUT1" x="15.24" y="7.62" visible="pin" length="middle" direction="pwr" rot="R180"/>
<pin name="VOUT2" x="15.24" y="2.54" visible="pin" length="middle" direction="pwr" rot="R180"/>
</symbol>
<symbol name="LM2931-ADJ">
<wire x1="-7.62" y1="7.62" x2="-7.62" y2="-7.62" width="0.254" layer="94"/>
<wire x1="-7.62" y1="-7.62" x2="10.16" y2="-7.62" width="0.254" layer="94"/>
<wire x1="10.16" y1="-7.62" x2="10.16" y2="7.62" width="0.254" layer="94"/>
<wire x1="10.16" y1="7.62" x2="-7.62" y2="7.62" width="0.254" layer="94"/>
<text x="-7.62" y="8.28" size="1.778" layer="95">&gt;NAME</text>
<text x="-7.62" y="-10.16" size="1.778" layer="96">&gt;VALUE</text>
<pin name="IN" x="-10.16" y="5.08" length="short" direction="pwr"/>
<pin name="ON" x="-10.16" y="0" length="short" direction="in"/>
<pin name="GND" x="-10.16" y="-5.08" length="short" direction="pwr"/>
<pin name="OUT" x="12.7" y="5.08" length="short" direction="out" rot="R180"/>
<pin name="ADJ" x="12.7" y="-5.08" length="short" direction="in" rot="R180"/>
</symbol>
<symbol name="LP2980">
<wire x1="-7.62" y1="5.08" x2="-7.62" y2="-5.08" width="0.254" layer="94"/>
<wire x1="-7.62" y1="-5.08" x2="10.16" y2="-5.08" width="0.254" layer="94"/>
<wire x1="10.16" y1="-5.08" x2="10.16" y2="5.08" width="0.254" layer="94"/>
<wire x1="10.16" y1="5.08" x2="-7.62" y2="5.08" width="0.254" layer="94"/>
<text x="-7.62" y="5.72" size="1.778" layer="95">&gt;NAME</text>
<text x="-7.62" y="-7.62" size="1.778" layer="96">&gt;VALUE</text>
<pin name="VIN" x="-10.16" y="2.54" length="short" direction="pwr"/>
<pin name="ON" x="-10.16" y="-2.54" length="short" direction="in"/>
<pin name="VOUT" x="12.7" y="2.54" length="short" direction="out" rot="R180"/>
<pin name="GND" x="12.7" y="-2.54" length="short" direction="pwr" rot="R180"/>
</symbol>
<symbol name="TLV00XX">
<wire x1="-7.62" y1="5.08" x2="7.62" y2="5.08" width="0.254" layer="94"/>
<wire x1="7.62" y1="5.08" x2="7.62" y2="-5.08" width="0.254" layer="94"/>
<wire x1="7.62" y1="-5.08" x2="-7.62" y2="-5.08" width="0.254" layer="94"/>
<wire x1="-7.62" y1="-5.08" x2="-7.62" y2="5.08" width="0.254" layer="94"/>
<text x="-7.62" y="6.35" size="1.27" layer="95">&gt;NAME</text>
<text x="-7.62" y="-7.366" size="1.27" layer="96">&gt;VALUE</text>
<pin name="VIN" x="-10.16" y="2.54" visible="pin" length="short" direction="sup"/>
<pin name="VOUT" x="10.16" y="2.54" visible="pin" length="short" direction="sup" rot="R180"/>
<pin name="EN" x="-10.16" y="-2.54" visible="pin" length="short"/>
<pin name="GND" x="10.16" y="-2.54" visible="pin" length="short" direction="sup" rot="R180"/>
</symbol>
<symbol name="V-REG-3-EN-ADJ">
<wire x1="-7.62" y1="-7.62" x2="7.62" y2="-7.62" width="0.4064" layer="94"/>
<wire x1="7.62" y1="-7.62" x2="7.62" y2="7.62" width="0.4064" layer="94"/>
<wire x1="7.62" y1="7.62" x2="-7.62" y2="7.62" width="0.4064" layer="94"/>
<wire x1="-7.62" y1="7.62" x2="-7.62" y2="-7.62" width="0.4064" layer="94"/>
<text x="-7.62" y="9.144" size="1.778" layer="95">&gt;NAME</text>
<text x="-7.62" y="-11.43" size="1.778" layer="96">&gt;VALUE</text>
<pin name="IN" x="-10.16" y="5.08" visible="pin" length="short" direction="in"/>
<pin name="GND" x="-10.16" y="0" visible="pin" length="short" direction="in"/>
<pin name="OUT" x="10.16" y="5.08" visible="pin" length="short" direction="pas" rot="R180"/>
<pin name="EN" x="-10.16" y="-5.08" visible="pin" length="short" direction="in"/>
<pin name="ADJ" x="10.16" y="-5.08" visible="pin" length="short" direction="in" rot="R180"/>
</symbol>
<symbol name="V-REG-3-EN-FIX">
<wire x1="-7.62" y1="-7.62" x2="7.62" y2="-7.62" width="0.4064" layer="94"/>
<wire x1="7.62" y1="-7.62" x2="7.62" y2="7.62" width="0.4064" layer="94"/>
<wire x1="7.62" y1="7.62" x2="-7.62" y2="7.62" width="0.4064" layer="94"/>
<wire x1="-7.62" y1="7.62" x2="-7.62" y2="-7.62" width="0.4064" layer="94"/>
<text x="-7.62" y="9.144" size="1.778" layer="95">&gt;NAME</text>
<text x="-7.62" y="-11.43" size="1.778" layer="96">&gt;VALUE</text>
<pin name="IN" x="-10.16" y="5.08" visible="pin" length="short" direction="in"/>
<pin name="GND" x="-10.16" y="0" visible="pin" length="short" direction="in"/>
<pin name="OUT" x="10.16" y="5.08" visible="pin" length="short" direction="pas" rot="R180"/>
<pin name="EN" x="-10.16" y="-5.08" visible="pin" length="short" direction="in"/>
<pin name="NC" x="10.16" y="-5.08" visible="pin" length="short" direction="in" rot="R180"/>
</symbol>
<symbol name="V-REG-3-FIX">
<description>3-pin voltage regulator</description>
<pin name="VIN" x="-7.62" y="2.54" visible="off" length="short"/>
<pin name="VOUT" x="7.62" y="2.54" visible="off" length="short" rot="R180"/>
<pin name="GND" x="0" y="-5.08" visible="off" length="short" rot="R90"/>
<wire x1="-5.08" y1="-2.54" x2="5.08" y2="-2.54" width="0.4064" layer="94"/>
<wire x1="5.08" y1="-2.54" x2="5.08" y2="5.08" width="0.4064" layer="94"/>
<wire x1="5.08" y1="5.08" x2="-5.08" y2="5.08" width="0.4064" layer="94"/>
<wire x1="-5.08" y1="5.08" x2="-5.08" y2="-2.54" width="0.4064" layer="94"/>
<text x="2.54" y="-5.08" size="1.778" layer="95">&gt;NAME</text>
<text x="2.54" y="-7.62" size="1.778" layer="96">&gt;VALUE</text>
<text x="-2.032" y="-1.778" size="1.524" layer="95">GND</text>
<text x="-4.445" y="1.905" size="1.524" layer="95">IN</text>
<text x="0.635" y="1.905" size="1.524" layer="95">OUT</text>
</symbol>
<symbol name="V-REG-3-FIX-HS">
<pin name="VIN" x="-7.62" y="2.54" visible="off" length="short"/>
<pin name="VOUT" x="7.62" y="2.54" visible="off" length="short" rot="R180"/>
<pin name="GND" x="0" y="-5.08" visible="off" length="short" rot="R90"/>
<wire x1="-5.08" y1="-2.54" x2="5.08" y2="-2.54" width="0.4064" layer="94"/>
<wire x1="5.08" y1="-2.54" x2="5.08" y2="5.08" width="0.4064" layer="94"/>
<wire x1="5.08" y1="5.08" x2="-5.08" y2="5.08" width="0.4064" layer="94"/>
<wire x1="-5.08" y1="5.08" x2="-5.08" y2="-2.54" width="0.4064" layer="94"/>
<text x="2.54" y="-5.08" size="1.778" layer="95">&gt;NAME</text>
<text x="2.54" y="-7.62" size="1.778" layer="96">&gt;VALUE</text>
<text x="-2.032" y="-1.778" size="1.524" layer="95">GND</text>
<text x="-4.445" y="1.905" size="1.524" layer="95">IN</text>
<text x="0.635" y="1.905" size="1.524" layer="95">OUT</text>
<pin name="HEATSINK" x="7.62" y="0" visible="off" length="short" rot="R180"/>
</symbol>
<symbol name="V-REG-3-FIX-TAB">
<pin name="VIN" x="-7.62" y="0" visible="off" length="short"/>
<pin name="VOUT" x="7.62" y="0" visible="off" length="short" rot="R180"/>
<pin name="GND" x="0" y="-7.62" visible="off" length="short" rot="R90"/>
<wire x1="-5.08" y1="-5.08" x2="5.08" y2="-5.08" width="0.4064" layer="94"/>
<wire x1="5.08" y1="-5.08" x2="5.08" y2="2.54" width="0.4064" layer="94"/>
<wire x1="5.08" y1="2.54" x2="-5.08" y2="2.54" width="0.4064" layer="94"/>
<wire x1="-5.08" y1="2.54" x2="-5.08" y2="-5.08" width="0.4064" layer="94"/>
<text x="2.54" y="-7.62" size="1.778" layer="95">&gt;NAME</text>
<text x="2.54" y="-10.16" size="1.778" layer="96">&gt;VALUE</text>
<text x="-2.032" y="-4.318" size="1.524" layer="95">GND</text>
<text x="-4.445" y="-0.635" size="1.524" layer="95">IN</text>
<text x="0.635" y="-0.635" size="1.524" layer="95">OUT</text>
<pin name="TAB" x="7.62" y="-2.54" visible="off" length="short" rot="R180"/>
</symbol>
<symbol name="V-REG-5-EN-PWRGD">
<wire x1="-7.62" y1="-7.62" x2="7.62" y2="-7.62" width="0.4064" layer="94"/>
<wire x1="7.62" y1="-7.62" x2="7.62" y2="7.62" width="0.4064" layer="94"/>
<wire x1="7.62" y1="7.62" x2="-7.62" y2="7.62" width="0.4064" layer="94"/>
<wire x1="-7.62" y1="7.62" x2="-7.62" y2="-7.62" width="0.4064" layer="94"/>
<text x="-5.08" y="9.144" size="1.778" layer="95">&gt;NAME</text>
<text x="-5.08" y="-11.43" size="1.778" layer="96">&gt;VALUE</text>
<pin name="IN" x="-10.16" y="5.08" visible="pin" length="short" direction="in"/>
<pin name="GND" x="-10.16" y="0" visible="pin" length="short" direction="in"/>
<pin name="OUT" x="10.16" y="5.08" visible="pin" length="short" direction="pas" rot="R180"/>
<pin name="EN" x="-10.16" y="-5.08" visible="pin" length="short" direction="in"/>
<pin name="PGD" x="10.16" y="-5.08" visible="pin" length="short" direction="in" rot="R180"/>
</symbol>
<symbol name="V-REG-5-EN-BYP">
<wire x1="-7.62" y1="7.62" x2="-7.62" y2="-7.62" width="0.254" layer="94"/>
<wire x1="-7.62" y1="-7.62" x2="7.62" y2="-7.62" width="0.254" layer="94"/>
<wire x1="7.62" y1="-7.62" x2="7.62" y2="7.62" width="0.254" layer="94"/>
<wire x1="7.62" y1="7.62" x2="-7.62" y2="7.62" width="0.254" layer="94"/>
<text x="-7.62" y="8.28" size="1.778" layer="95">&gt;NAME</text>
<text x="-7.62" y="-10.16" size="1.778" layer="96">&gt;VALUE</text>
<pin name="IN" x="-10.16" y="5.08" length="short" direction="pwr"/>
<pin name="EN" x="-10.16" y="0" length="short" direction="in"/>
<pin name="GND" x="-10.16" y="-5.08" length="short" direction="pwr"/>
<pin name="OUT" x="10.16" y="5.08" length="short" direction="out" rot="R180"/>
<pin name="BYP" x="10.16" y="-5.08" length="short" direction="in" rot="R180"/>
</symbol>
<symbol name="VREG">
<wire x1="-5.08" y1="-2.54" x2="5.08" y2="-2.54" width="0.4064" layer="94"/>
<wire x1="5.08" y1="-2.54" x2="5.08" y2="5.08" width="0.4064" layer="94"/>
<wire x1="5.08" y1="5.08" x2="-5.08" y2="5.08" width="0.4064" layer="94"/>
<wire x1="-5.08" y1="5.08" x2="-5.08" y2="-2.54" width="0.4064" layer="94"/>
<text x="2.54" y="-5.08" size="1.778" layer="95">&gt;NAME</text>
<text x="2.54" y="-7.62" size="1.778" layer="96">&gt;VALUE</text>
<text x="-2.032" y="-1.778" size="1.524" layer="95">GND</text>
<text x="-4.445" y="1.905" size="1.524" layer="95">IN</text>
<text x="0.635" y="1.905" size="1.524" layer="95">OUT</text>
<pin name="IN" x="-7.62" y="2.54" visible="off" length="short" direction="in"/>
<pin name="GND" x="0" y="-5.08" visible="off" length="short" direction="pwr" rot="R90"/>
<pin name="OUT" x="7.62" y="2.54" visible="off" length="short" direction="pas" rot="R180"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="MIC5320">
<description>&lt;b&gt;MIC5320 Dual ULDO Voltage Regulator&lt;/b&gt;
&lt;p&gt;The MIC5320 is a tiny Dual Ultra Low-Dropout (ULDO(TM)) linear regulator ideally suited for portable electronics.

&lt;p&gt;Reference: &lt;a href="http://www.micrel.com/_PDF/mic5320.pdf"&gt;http://www.micrel.com/_PDF/mic5320.pdf&lt;/a&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="MIC5320" x="0" y="0"/>
</gates>
<devices>
<device name="" package="SOT23-6">
<connects>
<connect gate="G$1" pin="EN1" pad="6"/>
<connect gate="G$1" pin="EN2" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VIN" pad="3"/>
<connect gate="G$1" pin="VOUT1" pad="4"/>
<connect gate="G$1" pin="VOUT2" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2931?-ADJ" prefix="IC">
<description>&lt;b&gt;&lt;a href=http://www.national.com&gt;National Semiconductor&lt;/a&gt; Low Dropout Adjustable Regulator&lt;/b&gt;&lt;p&gt;
Vout 3-24V, Vin up to 26V, Shutdown Pin, Reverse Batterie/Load Dump/Short Circuit/Overload Protection,</description>
<gates>
<gate name="A" symbol="LM2931-ADJ" x="0" y="0"/>
</gates>
<devices>
<device name="S" package="TO263-5">
<connects>
<connect gate="A" pin="ADJ" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="4"/>
<connect gate="A" pin="ON" pad="2"/>
<connect gate="A" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="T" package="TO220-5">
<connects>
<connect gate="A" pin="ADJ" pad="1"/>
<connect gate="A" pin="GND" pad="3"/>
<connect gate="A" pin="IN" pad="4"/>
<connect gate="A" pin="ON" pad="2"/>
<connect gate="A" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M" package="SO08">
<connects>
<connect gate="A" pin="ADJ" pad="4"/>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="IN" pad="8"/>
<connect gate="A" pin="ON" pad="5"/>
<connect gate="A" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="M-GNDPIN7" package="SO08">
<connects>
<connect gate="A" pin="ADJ" pad="4"/>
<connect gate="A" pin="GND" pad="7"/>
<connect gate="A" pin="IN" pad="8"/>
<connect gate="A" pin="ON" pad="5"/>
<connect gate="A" pin="OUT" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2980" prefix="IC">
<description>&lt;b&gt;&lt;a href=http://www.national.com&gt;National Semiconductor&lt;/a&gt; Micropower Linear Regulator&lt;/b&gt;&lt;p&gt;
50mA regulated output, Vin 16V max., ultra-low dropout of 120mV @ 50mA, 1µA standby current</description>
<gates>
<gate name="A" symbol="LP2980" x="0" y="0"/>
</gates>
<devices>
<device name="M5" package="SOT23-5">
<connects>
<connect gate="A" pin="GND" pad="2"/>
<connect gate="A" pin="ON" pad="3"/>
<connect gate="A" pin="VIN" pad="1"/>
<connect gate="A" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LP2980-ADJ">
<description>&lt;b&gt;LP2980IM5-ADJ&lt;/b&gt;

&lt;p&gt;50mA adjustable, ultra low drop out regulator in SOT-23-5 package&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="LM2931-ADJ" x="0" y="0"/>
</gates>
<devices>
<device name="-IM5" package="SOT23-5">
<connects>
<connect gate="G$1" pin="ADJ" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="ON" pad="3"/>
<connect gate="G$1" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TLV00XX">
<description>&lt;B&gt;TLV00XX, TLV01XX LDO Voltage Regulator&lt;/b&gt;
&lt;p&gt;The TLV700xx series of low-dropout (LDO) linear regulators are low quiescent current devices with excellent line and load transient performance. These LDOs are designed for power-sensitive applications.&lt;/p&gt;
&lt;p&gt;Datasheet: &lt;a href="http://www.ti.com/lit/ds/symlink/tlv70025.pdf"&gt;tlv70025.pdf&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="TLV00XX" x="0" y="0"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP1824" prefix="U">
<description>&lt;B&gt;MCP1824 LDO voltage regulator&lt;/B&gt;
&lt;p&gt;The MCP1824/MCP1824S is a 300 mA Low Dropout
(LDO) linear regulator that provides high current and
low output voltages. The MCP1824 comes in a fixed or
adjustable output voltage version, with an output
voltage range of 0.8V to 5.0V.&lt;/P&gt;
&lt;p&gt;&lt;a href="http://ww1.microchip.com/downloads/en/devicedoc/22070a.pdf"&gt;Datasheet.pdf&lt;/a&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="V-REG-3-EN-ADJ" x="0" y="0"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="G$1" pin="ADJ" pad="4"/>
<connect gate="G$1" pin="EN" pad="3"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP1801" prefix="U">
<description>&lt;b&gt;Microchip MCP1801 LDO Regulator&lt;/b&gt;

&lt;p&gt;The MCP1801 is a family of CMOS low dropout (LDO)
voltage regulators that can deliver up to 150 mA of
current while consuming only 25 μA of quiescent
current (typical) with input operating range from 2.0V to 10.0V.&lt;/p&gt;

&lt;p&gt;&lt;a href="http://ww1.microchip.com/downloads/en/DeviceDoc/22051D.pdf"&gt;Datasheet.pdf&lt;/a&gt;&lt;/p&gt;</description>
<gates>
<gate name="MCP1801" symbol="V-REG-3-EN-FIX" x="0" y="0"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="MCP1801" pin="EN" pad="3"/>
<connect gate="MCP1801" pin="GND" pad="2"/>
<connect gate="MCP1801" pin="IN" pad="1"/>
<connect gate="MCP1801" pin="NC" pad="4"/>
<connect gate="MCP1801" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LD29150" prefix="U">
<description>&lt;B&gt;STM LD29150 LDO Voltage Regulator&lt;/b&gt;
&lt;p&gt;The LD29150xx is a high current, high accuracy, 
low-dropout voltage regulator series. These 
regulators feature 400 mV dropout voltage and 
very low ground current. Designed for high 
current loads, these devices are also used in 
lower current, extremely low dropout-critical 
systems, where their tiny dropout voltage and 
ground current values are important attributes. &lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.st.com/web/en/resource/technical/document/datasheet/CD00003403.pdf"&gt;Datasheet.pdf&lt;/a&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="V-REG-3-FIX" x="0" y="0"/>
</gates>
<devices>
<device name="DT" package="DPAK">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP1825" prefix="U">
<description>&lt;b&gt;Microchip MCP1824 LDO Voltage Regulator&lt;/b&gt;
&lt;p&gt;The MCP1825/MCP1825S is a 500 mA Low Dropout
(LDO) linear regulator that provides high current and
low output voltages.&lt;/p&gt;

&lt;p&gt;&lt;a href="http://ww1.microchip.com/downloads/en/DeviceDoc/22056b.pdf"&gt;Datasheet.pdf&lt;/a&gt;&lt;/p&gt;</description>
<gates>
<gate name="&gt;NAME" symbol="V-REG-3-FIX-HS" x="0" y="0"/>
</gates>
<devices>
<device name="_SOT223" package="SOT-223-3">
<connects>
<connect gate="&gt;NAME" pin="GND" pad="2"/>
<connect gate="&gt;NAME" pin="HEATSINK" pad="4"/>
<connect gate="&gt;NAME" pin="VIN" pad="1"/>
<connect gate="&gt;NAME" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LF50CDT" prefix="U">
<description>&lt;b&gt;5V LDO Voltage Regulator&lt;/b&gt;
&lt;p&gt;The LFxxAB/LFxxC are very low drop regulators 
available in PENTAWATT, TO-220, TO-220FP, 
DPAK and PPAK package and in a wide range of 
output voltages.&lt;/p&gt;&lt;p&gt;The very low drop voltage (0.45 
V) and the very low quiescent current make them 
particularly suitable for low noise, low power 
applications and specially in battery powered 
systems&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.st.com/web/en/resource/technical/document/datasheet/CD00000546.pdf"&gt;Datasheet.pdf&lt;/a&gt;&lt;/p&gt;</description>
<gates>
<gate name="LF50CDT" symbol="V-REG-3-FIX" x="0" y="0"/>
</gates>
<devices>
<device name="" package="DPAK">
<connects>
<connect gate="LF50CDT" pin="GND" pad="4"/>
<connect gate="LF50CDT" pin="VIN" pad="1"/>
<connect gate="LF50CDT" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM2940" prefix="U">
<description>&lt;b&gt;LM2940 LDO Voltage Regulator&lt;/b&gt;

&lt;p&gt;The LM2940-N/LM2940C positive voltage regulator features the ability to source 1A of output current with a dropout voltage of typically 0.5V and a maximum of 1V over the entire temperature range. Furthermore, a quiescent current reduction circuit has been included which reduces the ground current when the differential between the input voltage and the output
exceeds approximately 3V.&lt;/p&gt;

&lt;p&gt;Designed also for vehicular applications, the LM2940-N/LM2940C and all regulated circuitry are protected from reverse battery installations or 2-battery jumps. During line transients, such as load dump when the
input voltage can momentarily exceed the specified maximum operating voltage, the regulator will automatically shut down to protect both the internal circuits and the load. The LM2940/LM2940C cannot be harmed by temporary mirror-image insertion.
Familiar regulator features such as short circuit and thermal overload protection are also provided.&lt;/p&gt;

&lt;p&gt;&lt;a href="http://www.ti.com/lit/ds/symlink/lm2940-n.pdf"&gt;Datasheet.pdf&lt;/a&gt;&lt;/p.</description>
<gates>
<gate name="G$1" symbol="V-REG-3-FIX-TAB" x="0" y="2.54"/>
</gates>
<devices>
<device name="DCY" package="SOT-223-3">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="TAB" pad="4"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="KTT" package="TO263-3">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="TAB" pad="4"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NDE" package="TO220L1">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="TAB" pad="4"/>
<connect gate="G$1" pin="VIN" pad="1"/>
<connect gate="G$1" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP1755" prefix="IC">
<description>&lt;b&gt;Microchip MCP1755 LDO Voltage Regulator&lt;/b&gt;
&lt;p&gt;The MCP1755/1755S is a family of CMOS low-dropout
(LDO) voltage regulators that can deliver up to 300 mA
of current while consuming only 68.0 μA of quiescent
current (typical). The input operating range is specified
from 3.6V to 16.0V, making it an ideal choice for four to
six primary cell battery-powered applications, 12V
mobile applications and one to three cell Li-Ion-
powered applications.&lt;/p&gt;
&lt;a href="http://ww1.microchip.com/downloads/en/DeviceDoc/25160A.pdf"&gt;datasheet.pdf&lt;/a&gt;</description>
<gates>
<gate name="U1" symbol="V-REG-5-EN-PWRGD" x="0" y="0"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="U1" pin="EN" pad="3"/>
<connect gate="U1" pin="GND" pad="2"/>
<connect gate="U1" pin="IN" pad="1"/>
<connect gate="U1" pin="OUT" pad="5"/>
<connect gate="U1" pin="PGD" pad="4"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NCP5500" prefix="U">
<description>&lt;b&gt;NCP5500, NCV5500, NCP5501, NCV5501 LDO Voltage Regulator&lt;/b&gt;
&lt;p&gt;These linear low drop voltage regulators provide up to 500 mA over
a user−adjustable output range of 1.25 V to 5.0 V, or at a fixed output
voltage of 1.5 V, 3.3 V or 5.0 V, with typical output voltage accuracy
better than 3%. Reverse bias protection, thermal shutdown, and short
circuit protection. Dropout is 230 mV at 500 mA&lt;/p&gt;</description>
<gates>
<gate name="U1" symbol="V-REG-3-FIX" x="0" y="-2.54"/>
</gates>
<devices>
<device name="" package="DPAK">
<connects>
<connect gate="U1" pin="GND" pad="4"/>
<connect gate="U1" pin="VIN" pad="1"/>
<connect gate="U1" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="TC1262" prefix="U">
<description>&lt;b&gt;Microchip TC1262 LDO Regulator&lt;/b&gt;
&lt;p&gt;
The TC1262 is a fixed output, high accuracy (typically
±0.5%) CMOS low dropout regulator. Designed specif-
ically for battery-operated systems, the TC1262’s
CMOS construction eliminates wasted ground current,
significantly extending battery life. Total supply current
is typically 80A at full load (20 to 60 times lower than
in bipolar regulators).&lt;/p&gt;
&lt;p&gt;TC1262 key features include ultra low noise operation,
very low dropout voltage (typically 350mV at full load),
and fast response to step changes in load.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://ww1.microchip.com/downloads/en/DeviceDoc/21373C.pdf"&gt;Datasheet.pdf&lt;/a&gt;&lt;/p&gt;</description>
<gates>
<gate name="U1" symbol="V-REG-3-FIX-TAB" x="0" y="0"/>
</gates>
<devices>
<device name="_VDB" package="SOT-223-3">
<connects>
<connect gate="U1" pin="GND" pad="2"/>
<connect gate="U1" pin="TAB" pad="4"/>
<connect gate="U1" pin="VIN" pad="1"/>
<connect gate="U1" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_VAB" package="TO220L1">
<connects>
<connect gate="U1" pin="GND" pad="2"/>
<connect gate="U1" pin="TAB" pad="4"/>
<connect gate="U1" pin="VIN" pad="1"/>
<connect gate="U1" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_VEB" package="D2PACK-3">
<connects>
<connect gate="U1" pin="GND" pad="2"/>
<connect gate="U1" pin="TAB" pad="4"/>
<connect gate="U1" pin="VIN" pad="1"/>
<connect gate="U1" pin="VOUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MIC5205" prefix="IC">
<description>&lt;b&gt;ULDO Voltage regulator&lt;/b&gt;
&lt;p&gt;The MIC5205 is an efficient linear voltage regulator with ultra low-noise output, very low dropout voltage (typically 17mV at light loads and 165mV at 150mA), and very low ground current (600⎧A at 100mA output). The MIC5205 offers better than 1% initial accuracy.&lt;/p&gt;
&lt;p&gt;Designed especially for hand-held, battery-powered devices, the MIC5205 includes a CMOS or TTL compatible enable/shutdown control input. When shut down, power consumption drops nearly to zero. Regulator ground current increases only slightly in dropout, further prolonging battery life.&lt;/p&gt;
&lt;p&gt;Key MIC5205 features include a reference bypass pin to improve its already excellent low-noise performance, reversed-battery protection, current limiting, and overtemperature shutdown.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.micrel.com/_PDF/mic5205.pdf"&gt;datasheet.pdf&lt;/a&gt;</description>
<gates>
<gate name="MIC5205" symbol="V-REG-5-EN-BYP" x="0" y="0"/>
</gates>
<devices>
<device name="" package="SOT23-5">
<connects>
<connect gate="MIC5205" pin="BYP" pad="4"/>
<connect gate="MIC5205" pin="EN" pad="3"/>
<connect gate="MIC5205" pin="GND" pad="2"/>
<connect gate="MIC5205" pin="IN" pad="1"/>
<connect gate="MIC5205" pin="OUT" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="L4941" prefix="IC">
<description>&lt;B&gt;LD4941 LDO 1A Regulator&lt;/B&gt;
&lt;p&gt;ST Microelectronics&lt;/p&gt;
&lt;p&gt;The L4941 is a three terminal 5V positive 
regulators available in TO-220 and DPAK 
packages, making it useful in a wide range of 
industrial and consumer applications. Thanks to 
its very low input/output voltage drop, these 
devices are particularly suitable for battery 
powered equipments, reducing consumption and 
prolonging battery life. It employs internal current 
limiting, antisaturation circuit, thermal shut-down 
and safe area protection.&lt;/p&gt;
&lt;p&gt;Reference: &lt;a href="http://www.st.com/stonline/books/pdf/docs/2142.pdf"&gt;http://www.st.com/stonline/books/pdf/docs/2142.pdf&lt;/a&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="VREG" x="0" y="0"/>
</gates>
<devices>
<device name="BDT-TR" package="DPAK">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BV" package="TO220BV">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="BH" package="TO220BH">
<connects>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="IN" pad="1"/>
<connect gate="G$1" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1117" prefix="IC">
<description>&lt;b&gt;LDO Voltage Regulator&lt;/b&gt;

&lt;p&gt;NCP1117 series are low dropout positive voltage regulators that are capable of providing an output current that is in excess of 1.0 A with a maximum dropout voltage of 1.2 V at 800 mA over
temperature. This series contains nine fixed output voltages of 1.5 V, 1.8 V, 1.9 V, 2.0 V, 2.5 V, 2.85 V, 3.3 V, 5.0 V, and 12 V that have no minimum load requirement to maintain regulation. Also included is an adjustable output version that can be programmed from 1.25 V to 18.8 V with two external resistors. &lt;a href="http://www.onsemi.com/pub_link/Collateral/NCP1117-D.PDF"&gt;datasheet.pdf&lt;/a&gt;

&lt;p&gt;LM1117-N is a series of low dropout voltage regulators of 1.2V at 800mA of load current. It has the same pin-out as Texas Instruments' industry standard LM317. The LM1117-N is available in an adjustable version, available in five fixed voltages, 1.8V, 2.5V, 2.85V, 3.3V, and 5V. The LM1117-N offers current limiting and thermal shutdown. Its circuit includes a zener trimmed to within ±1%.
&lt;a href="http://www.ti.com/lit/ds/symlink/lm1117-n.pdf"&gt;datasheet.pdf&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="V-REG-3-FIX-HS" x="0" y="0"/>
</gates>
<devices>
<device name="-SOT223" package="SOT-223-3">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="HEATSINK" pad="4"/>
<connect gate="G$1" pin="VIN" pad="3"/>
<connect gate="G$1" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-TO22OH" package="TO220L1">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="HEATSINK" pad="4"/>
<connect gate="G$1" pin="VIN" pad="3"/>
<connect gate="G$1" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM1117-MOD">
<gates>
<gate name="G$1" symbol="V-REG-3-FIX" x="0" y="0"/>
</gates>
<devices>
<device name="" package="TO220BV">
<connects>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="VIN" pad="3"/>
<connect gate="G$1" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
